# 1 "/opt/topspin/exp/stan/nmr/lists/pp/user/zg30"
;zg30
;avance-version (02/05/31)
;1D sequence
;using 30 degree flip angle


;$OWNER=nmrsu
# 1 "/opt/topspin/exp/stan/nmr/lists/pp/Avance.incl" 1
;Avance2.incl
;   for 1
;
;avance-version (07/08/21)
;
;$CLASS=HighRes Incl
;$COMMENT=





































































































































;$Id: Avance2.incl,v 1.17.2.1 2007/09/14 16:17:35 ber Exp $
# 8 "/opt/topspin/exp/stan/nmr/lists/pp/user/zg30" 2



# 1 "mc_line 11 file /opt/topspin/exp/stan/nmr/lists/pp/user/zg30 expanding definition part of mc command before ze"
define delay MCWRK
define delay MCREST
"MCWRK = 0.333333*30m"
"MCREST = 30m - 30m"
    dccorr
# 11 "/opt/topspin/exp/stan/nmr/lists/pp/user/zg30"
1 ze
# 1 "mc_line 11 file /opt/topspin/exp/stan/nmr/lists/pp/user/zg30 expanding definition of mc command after ze"
# 12 "/opt/topspin/exp/stan/nmr/lists/pp/user/zg30"
# 1 "mc_line 12 file /opt/topspin/exp/stan/nmr/lists/pp/user/zg30 expanding start label for mc command"
2 MCWRK  * 2
LBLF0, MCWRK
  MCREST
# 13 "/opt/topspin/exp/stan/nmr/lists/pp/user/zg30"
  d1
  p1*0.33 ph1
  go=2 ph31
# 1 "mc_line 16 file /opt/topspin/exp/stan/nmr/lists/pp/user/zg30 expanding mc command in line"
  MCWRK wr #0
  MCWRK zd 
  lo to LBLF0 times td0

  MCWRK
# 17 "/opt/topspin/exp/stan/nmr/lists/pp/user/zg30"
exit


ph1=0 2 2 0 1 3 3 1
ph31=0 2 2 0 1 3 3 1


;pl1 : f1 channel - power level for pulse (default)
;p1 : f1 channel -  90 degree high power pulse
;d1 : relaxation delay; 1-5 * T1
;NS: 1 * n, total number of scans: NS * TD0



;$Id: zg30,v 1.7 2002/06/12 09:05:20 ber Exp $
